Fasten Safety Belt Indicator/Chime Always On. Chevrolet PJJ 2000

For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you perform the Instrument Cluster Diagnostic System Check? | Go to Step 2 | Go to A Diagnostic System Check - Instrument Cluster

2

1. Install a scan tool.
2. Turn ON the ignition, with the engine OFF.
3. Buckle the driver's seat belt.
4. With a scan tool, observe the DRIVER SIDE BELT STATUS parameter in the SIR data list.

Does the scan tool display UNBUCKLED?

Go to Step 3

Go to Testing for Intermittent and Poor Connections in Wiring Systems

3 | Disconnect the seat belt switch. Does the scan tool still display UNBUCKLED? | Go to Step 4 | Go to Step 5

4

1. Turn OFF the ignition.
2. Unbuckle the driver's seat belt.
3. Disconnect the seat belt switch.
4. Test the seat belt switch signal circuit for a short to ground.

Did you find and correct the condition?

Go to Step 7

Go to Step 6

5 | Replace the seat belt switch. Did you complete the replacement? | Go to Step 7 | --
6 | Replace the SDM. Refer to Inflatable Restraint Sensing and Diagnostic Module Replacement in SIR. Did you complete the replacement? | Go to Step 7 | --
7 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 2