Windshield Pillar Garnish Molding Replacement. Chevrolet PJJ 2001

For 1990-2009 cars

### Removal Procedure

1. Pull the windshield upper garnish molding (2 or 3) at the roof in order to disengage the clips.
2. Pull the windshield upper garnish molding (2 or 3) upward in order to disengage the molding from the carpet retainer.

### Installation Procedure

1. Insert the windshield upper garnish molding (2 or 3) into the carpet retainer.
2. Push the windshield upper garnish molding (2 or 3) in order to engage the clips.