Headlining Trim Panel Replacement. Chevrolet PJJ 2001

For 1990-2009 cars

The one-piece formed headlining trim finish panel consists of molded substrate covered with a foam backed cloth. Install the following components in order to install the headlining trim finish panel:

• | The related hardware

• | The interior moldings

The headlining trim finish panel is a one-piece construction. Service the panel as a complete assembly.

### Removal Procedure

1. Remove the assist strap.
2. Remove the sunshades. Refer to Sunshade Replacement.
3. Remove the coat hooks. Refer to Coat Hook Replacement.
4. Remove the windshield upper garnish moldings. Refer to Garnish Molding Replacement - Windshield Pillar.
5. Remove the center pillar upper trim panels. Refer to Garnish Molding Replacement - Center Pillar.
6. Remove the quarter trim panel. Refer to Trim Panel Replacement - Rear Quarter (2 Door) or Trim Panel Replacement - Rear Quarter (4 Door) .
7. Remove the finish lace from the sunroof opening trim, if equipped. Refer to Finishing Lace Replacement in Roof.
8. Remove the retainers from the headlining trim finish panel (3).
9. Remove the headlining trim finish panel (1).
10. Disconnect the wire harness from the headlining trim finish panel.

### Installation Procedure

1. Use adhesive tape GM P/N 9986080 in order to connect the wire harness to the headlining trim finish panel.

Important: Use care when loading the headlining into the vehicle. Flexing may cause damage to the headlining.

2. Install the headlining trim finish panel (1).
3. Install the retainers to the headlining trim finish panel(3).
4. Install the finish lace to the sunroof opening trim, if equipped. Refer to Finishing Lace Replacement .
5. Install the quarter trim panel. Refer to Trim Panel Replacement - Rear Quarter (2 Door) orTrim Panel Replacement - Rear Quarter (4 Door) for 4 door.
6. Install the center pillar upper trim panels. Refer to Garnish Molding Replacement - Center Pillar.
7. Install the windshield upper garnish molding. Refer to Garnish Molding Replacement - Windshield Pillar.
8. Install the coat hooks. Refer to Coat Hook Replacement.
9. Install the sunshades. Refer to Sunshade Replacement.
10. Install the assist strap.