Aluminum Wheel Hub Cap Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the tire and the wheel assembly. Refer to Tire and Wheel Removal and Installation.
2. Use a flat tip screwdriver in order to remove the hub cap.

### Installation Procedure

1. Install the hub cap by centering on the wheel and tapping gently until the hub cap is firmly seated.
2. Install the tire and the wheel assembly. Refer to Tire and Wheel Removal and Installation.