Front Door Inside Handle Rod Replacement. Chevrolet PJJ 2001

For 1990-2009 cars

### Removal Procedure

1. Raise the window to the full UP position.
2. Remove the door trim panel. Refer to Trim Panel Replacement - Door.
3. Remove the inside handle rivet.
4. Slide the inside handle rearward in order to disengage the tabs.
5. Remove both rods from the inside door handle. The rods are identified by the following colors:

• | The left hand rod (3) is red.

• | The right hand rod (2) is green.

6. Remove the door water deflector in order access the door lock assembly. Refer to Water Deflector Replacement - Door.
7. Remove the door lock assembly. Refer to Lock Replacement - Door.

### Installation Procedure

1. Install the door lock assembly. Refer to Lock Replacement - Door.
2. Install the door water deflector. Refer to Water Deflector Replacement - Door.
3. Install both rods to the inside door handle. The rods are identified by color as follows:

• | The left hand rod is red (3).

• | The right hand rod is green (2).

4. Slide the inside handle forward in order to engage the tabs.
5. Install the inside handle rivet.
6. Install the door trim panel. Refer to Trim Panel Replacement - Door.