Starter Solenoid Does Not Click. Chevrolet PJJ 2000

For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you perform the Diagnostic System Check for starting and charging? | Go to Step 2 | Go to Diagnostic System Check - Charging System Diagnostic System Check for starting and charging
2 | Turn the ignition to the START position. Does the starter solenoid click? | Go to Step 3 | Go to Step 5
3 | Did the engine crank and run? | Go to Symptoms | Go to Step 4
4 | Did the engine crank, run and stall? | Go to Diagnostic System Check - Theft Deterrent in Theft Deterrent | --

5

1. Turn OFF the ignition.
2. Disconnect the crank signal circuit to the starter solenoid.
3. Connect a test lamp between the crank signal circuit of the starter and a good ground.
4. Turn the ignition to the START position.

Does the test lamp illuminate?

Go to Step 7

Go to Step 6

6 | Test the control circuit of the starter solenoid for a high resistance or an open. Refer to Circuit Testing and Wiring Repairs in Wiring Systems. Did you find and correct the condition? | System OK | Go to Step 9
7 | Inspect for poor connections at the ignition switch. Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairs in Wiring Systems. Did you find and correct the condition? | System OK | Go to Step 8
8 | Inspect for poor connections at the starter solenoid. Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairs in Wiring Systems. Did you find and correct the condition? | System OK | Go to Step 10
9 | Replace the Ignition Switch. Refer to Ignition Switch Replacement - On Vehicle in Steering Wheel and Column -Tilt . Did you complete the replacement? | Go to Step 11 | --
10 | Replace the Starter Motor. Refer to Starter Motor Replacement . Did you complete the replacement? | Go to Step 11 | --
11 | Operate the system for which the symptom occurred. Is the symptom still present? | Go to Diagnostic System Check - Charging System | System OK