Shock Absorber Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the lower mounting bolt (5) from the shock absorber (5).
2. Remove the bolt (2) and the nuts (1) from the shock absorber (6).

### Installation Procedure

1. Install the nuts (1) and the bolt (2) to the shock absorber (6).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the lower nut from the shock absorber.

Tighten

• | Tighten the nuts to 25 N·m (18 lb ft).

• | Tighten the bolt to 25 N·m (18 lb ft).

3. Install the lower mounting bolt (5) to the shock absorber (6).

Tighten
Tighten the bolt to 70 N·m (52 lb ft).