Side Cover Axle Seal Installation. Chevrolet PJJ 1999

For 1990-2009 cars

#### Tools Required

• | J 8092 Driver Handle

• | J 41102-1A Axle Seal Installer

Important: You must use the J 41102-1A in order to install the seal correctly. The J 41102-1A installs the axle seal to a given depth.

1. Install a new side cover axle seal (2) into the side cover. Use the J 41102-1A with the J 8092 .
2. In order to prevent damage to the shaft splines during vehicle operation, add Polyurea grease (part number 7843867) to the splines on the output shaft.