Rear Seat Belt Buckle Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the seat cushion. Refer to Seat Cushion Replacement - Rear in Seats.
2. Remove the seat belt buckle anchor bolt.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the anchor bolts.

Tighten
Tighten the anchor bolts to 41 N·m (30 lb ft).

2. Install the seat cushion. Refer to Seat Cushion Replacement - Rear in Seats.