SMU - Revised Instrument Panel Cluster (IPC) Replacement. Chevrolet PJJ 1999

For 1990-2009 cars

# SMU - Revised Instrument Panel Cluster (IPC) Replacement

Subject: | Revised Instrument Panel Cluster (IPC) Replacement

Models: | 1995 Chevrolet Cavalier with 2.3L Engine (VIN D - RPO LD2)

| 1995 Pontiac Sunfire with 2.3L Engine (VIN D - RPO LD2)

| 1996-1999 Chevrolet Cavalier

| 1996-1999 Pontiac Sunfire

| 1996-1999 Toyota Cavalier

This bulletin is being issued to add a step to the Instrument Panel Cluster (IPC) Replacement procedure in the Instrument Panel and Console sub-section of the Service Manual. Please add this information to your Service Manual.

The following information has been updated within SI2000. If you are using a paper version of this Service Manual, please make a reference to this bulletin on the affected page.

It is necessary to reprogram the theft deterrent system after IPC replacement. The final step of the installation procedure of the Instrument Panel Cluster (IPC) Replacement procedure should read "Disengage the theft deterrent tamper mode. Refer to PASSLOCK Changing - Components Description in Theft Deterrent."