Body Tail Lamp Filler Panel Replacement. Chevrolet PJJ 2001

For 1990-2009 cars

### Removal Procedure

1. Remove the tail lamp filler panel nuts (1).
2. Remove the tail lamp filler panel (2).
3. Remove the seal washer (2).

### Installation Procedure

1. Install the seal washer (2) to the tail lamp filler panel.
2. Install the tail lamp filler panel (2).
3. Align the tail lamp filler panel to the rear compartment deck lid.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the tail lamp filler panel nuts (1).

Tighten
Tighten the filler panel nuts to 6 N·m (53 lb in).