Intermediate Steering Shaft Seal Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the intermediate steering shaft. Refer to Intermediate Steering Shaft Replacement.
2. Remove the intermediate steering shaft seal from the front of dash panel.
3. Remove the intermediate steering shaft seal from the vehicle.

### Installation Procedure

Caution: If steering column to cowl panel seal is torn or otherwise damaged, it must be replaced. Confirm that the seal and inner race are properly located. Failure to do so may allow carbon monoxide into the vehicle, which may result in serious personal injury or death.

1. Install the intermediate steering shaft seal to the vehicle.
2. Position the intermediate steering shaft seal on the front of dash panel.
3. Install the intermediate steering shaft. Refer to Intermediate Steering Shaft Replacement.