Battery Positive Cable Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Disconnect the positive battery cable at the battery.
3. Cut the tape holding the two cables together at the retainer on the battery tray.
4. Cut the tape holding the two cables together near the transmission electical plug.
5. Remove the positive battery cable nut at the starter solenoid. Refer to Starter Motor Replacement .
6. Remove the positive battery cable from the vehicle.

### Installation Procedure

1. Position the new cable in the vehicle in the same location as the old cable.
2. Install the cable end onto the starter. Refer to Starter Motor Replacement .
3. Tape the cables together at the transmission electrical connector.
4. Tape the cables together at the battery tray.
5. Install the positive battery cable end onto the battery.
6. Tighten the positive battery cable bolt to the battery to 20 N·m (15 lb ft).
7. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .