Fastener Tightening Specifications. Chevrolet PJJ 2000

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Adjuster Plug Locknut | 70 N·m | 50 lb ft
Crossmember Support Bolts | 110 N·m | 71 lb ft
Pinion Locknut | 35 N·m | 26 lb ft
Pinion Preload | 2 N·m | 16 lb in
Power Steering Gear Mounting Bolts | 120 N·m | 89 lb ft
Power Steering Hose Fitting | 27 N·m | 20 lb ft
Power Steering Pump Mounting Bolt | 26 N·m | 19 lb ft
Power Steering Return Hose Retainer Nut | 13 N·m | 10 lb ft
Rack and Pinion Cylinder Line Fittings at Cylinder End | 28 N·m | 21 lb ft
Rack and Pinion Cylinder Line Fittings at Valve End | 27 N·m | 20 lb ft
Rack and Pinion Cylinder Line Fittings at Cylinder End | 28 N·m | 21 lb ft
Tie Rod Ball Stud Nut | 45 N·m | 33 lb ft
Tie Rod Jam Nut | 68 N·m | 50 lb ft