Inflatable Restraint Coil Centering - Off Vehicle. Chevrolet PJJ 2000

For 1990-2009 cars

Important: A new SRS coil assembly will be pre-centered.

Improper alignment of the SRS coil assembly may damage unit causing an inflatable restraint malfunction.
1. Verify the following before centering the SRS coil assembly:

• | The wheels on the vehicle are straight ahead.

• | The block tooth (1) of the steering shaft assembly is in the 12 o' clock position.

• | The ignition switch is in the "LOCK" position.

2. If the front (4) of the SRS coil has a centering window (3) and no spring service lock on the back side (1), perform the following steps:

2.1. | Hold the coil assembly with the face up.

2.2. | Rotate the coil hub clockwise until the coil ribbon can no longer travel.

2.3. | Rotate the coil hub slowly, counter clockwise until the centering window appears yellow and both arrows (2) line up. This is center position.

2.4. | While holding the coil hub in center position, align the SRS coil assembly with the horn tower and slide onto steering shaft assembly.