Front Seats Description. Chevrolet PJJ 2000

For 1990-2009 cars

All coupe body styles are equipped with bucket seats. The bucket seats contain a manual lock system. Manually release the seat back as desired in order to provide easier access to the rear seat. The manual lock system is part of the recliner mechanism. The recliner mechanism mounts on the outboard side of the front seat.

The manually operated front adjusters provide forward and rearward movement of the seat. Actuating the seat control lever unlocks the seat adjusters. This permits travel of the seat. The seat locks into place under the following conditions:

• | The seat is in the desired position.

• | The seat control lever is released.

The driver's seat buckle side belt attaches to the seat adjuster assembly. The driver's seat is a load bearing seat.

### Passenger Front E-Z Entry

The passenger front seat E-Z entry system has the adjuster release lever located on the outer adjuster. The inner adjuster acts as a slave unit. Perform the following steps in order to activate the inner adjuster:

• | Lift the seat back latch.

• | Move the seat back forward.

When you enter the rear seating area, the forward movement of the seat back trips a cable. The cable releases a lock bar on the adjuster. This action allows the seat to move forward in order to provide more room for passenger entry into the rear seat.

Apply rearward pressure to the top of the seat back in order to return the seat to the original position. The seat moves rearward until the E-Z entry lock feature engages.

Normal seat adjuster travel is 180 mm (7 in) from the full rear position to the full forward position. The E-Z entry adjuster travel is 140 mm (5.5 in) when the seat is in the full-rear position.