Rattle in Rack and Pinion Steering Gear. Chevrolet PJJ 2000

For 1990-2009 cars

Condition | Action
--- | ---

The power steering gear inlet (pressure) hose is grounding out.

Inspect the power steering gear inlet (pressure) hose. Determine if the following items are correct:

• | The mounting

• | The clearance

Refer to Power Steering Pressure Hose Replacement.

The rack bearing adjust is loose. | Tighten the rack bearing adjust to specification. Refer to to Fastener Tightening Specifications.
The steering gear is loose. | Tighten the steering gear mounting bolts to specification. Refer to Power Steering Pressure Hose Replacement.

The tie rod ends are loose.

1. Inspect the tie rod ends.
2. Replace the tie rod ends as needed.

Refer to Tie Rod End Replacement - Outer - On Vehicle.

The intermediate steering shaft is loose. | Tighten the upper or lower intermediate steering shaft bolt to specification. Refer to Fastener Tightening Specifications.