Fuel Tank Filler Pipe Housing Replacement. Chevrolet PJJ 2001

For 1990-2009 cars

### Removal Procedure

1. Remove the fuel tank filler door. Refer to Fuel Filler Door Replacement.
2. Remove the filler door latch. Refer to Fuel Filler Door Release Actuator Replacement.
3. Remove the bolts (2) from the fuel tank filler pocket.
4. Remove the fuel tank filler pocket (1).

### Installation Procedure

1. Install the fuel tank filler pocket (1).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the bolts (2) to the fuel tank filler pocket.

Tighten
Tighten the bolts to 2 N·m (24 lb in).

3. Install the filler door latch. Refer to Fuel Filler Door Release Actuator Replacement .
4. Install the fuel tank filler door. Refer to Fuel Filler Door Replacement.