Power Sunroof Express Module Replacement. Chevrolet PJJ 2001

For 1990-2009 cars

### Removal Procedure

1. Close the sunroof.
2. Remove the sunroof trim lace (1). Refer to Sunroof Opening Trim Finish Lace Replacement .
3. Remove the sunroof sunshade. Refer to Sunroof Sunshade Replacement .
4. Remove the headliner trim finish panel (3) as required. Refer to Headlining Trim Panel Replacement in interior trim.

• | Disconnect the sunroof control switch

• | Disconnect the dome lamp connector

5. Remove the express module from the vehicle by sliding the express module (8) towards the middle of the vehicle.
6. Disconnect the wire harness connectors from the express module (8).

### Installation Procedure

1. Connect the wire harness connectors to the express module (8).
2. Install the express module into the vehicle by sliding the express module (8) towards the left side of the vehicle.
3. Install the headliner. Refer to Headlining Trim Panel Replacement in interior trim.

• | Connect the sunroof control switch

• | Connect the dome lamp

4. Install the sunroof opening trim lace (1). Refer to Sunroof Opening Trim Finish Lace Replacement .
5. Install the sunroof sunshade. Refer to Sunroof Sunshade Replacement .