Fog Lamp Relay Replacement. Chevrolet PJJ 2001

For 1990-2009 cars

### Removal Procedure

1. Remove the upper air intake splash shield. Refer to Hood Close Out Filler Replacement in Body Front End.
2. Remove the fog lamp relay fastener (1) from behind the left side of the front impact bar.
3. Disconnect the electrical connector (2).
4. Remove the relay (3).

### Installation Procedure

1. Connect the electrical connector (2).
2. Install the relay fastener.
3. Install the upper air intake splash shield. Refer to Hood Close Out Filler Replacement in Body Front End.