Console Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

1. Open the console compartment (1).
2. Remove gear shift handle.
3. Refer to Trim Plate Replacement - Console in order to remove the power window trim plate.
4. Disconnect electrical connectors.
5. Remove the screw cover from inside the console (1).
6. Remove the screws (2).
7. Remove the console.
8. Disconnect electrical connectors.

### Installation Procedure

1. Connect the electrical connectors.
2. Install the console.
3. Install the screws (2).

Tighten
Tighten the screws to 2 N·m (18 lb in).

4. Install the console compartment screw cover (1) from inside the console compartment.
5. Refer to Trim Plate Replacement - Console in order to install the power window trim plate.
6. Close the console compartment.