Rear Window Trim Finish Panel Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

1. Lower the rear seatback.
2. Remove the rear quarter trim panel. Refer to Trim Panel Replacement - Rear Quarter in Interior Trim.
3. Remove the rear window trim panel retainers (2).
4. Remove the rear seat belts through the slot in the rear window trim panel.
5. Remove the rear window trim panel (1).

### Installation Procedure

1. Install the rear seat belts through the slot in the rear window trim panel.
2. Align the rear seatback striker through the slot in the rear window trim panel.
3. Install the rear window trim panel (1).
4. Install the rear window trim panel retainers (2).
5. Install the rear quarter trim panel. Refer to Trim Panel Replacement - Rear Quarter in Interior Trim.
6. Raise the rear seatback.