Squeaks and Rattles. Chevrolet PJJ 2000

For 1990-2009 cars

Improperly controlled relative motion between vehicle components causes squeaks and rattles. The following 3 measures may prevent a squeak or a rattle:

• | Attach the components securely. Ensure that there is no relative motion during operation of the vehicle.

• | Separate the components. Ensure that there is no contact under vehicle operating conditions.

• | Insulate the components in order to ensure that squeaks or rattles do not occur with relative motion between the vehicle components.

| Low uniform friction surfaces may eliminate "stick-slip" motion.