Info - ReAttachment Procedure for Loose Power Outside Rearview Mirror Module. Chevrolet PJJ 1999

For 1990-2009 cars

# Info - ReAttachment Procedure for Loose Power Outside Rearview Mirror Module

Subject: | Reattachment Procedure for Loose Power Outside Rearview Mirror Module

Models: | 1996-2000 Toyota Cavalier

If a condition is encountered where the power folding outside rearview mirror module, attached to the right side kick panel area, becomes disengaged from the original attachment, reattach the module to the original mount and use plastic tie straps to provide additional support using the following procedure:

• | Place one plastic tie strap around the wiring harness for the power folding mirror module, just below the connector.

• | Using two additional tie straps, loop them through the first tie strap, in front of the module and over the dash wiring harness, which is located above the power folding mirror module. The power folding mirror module is then supported by the dash wiring harness and held to the right side kick panel by the original attachment.