Fog Lamp Indicator Inoperative. Chevrolet PJJ 2000

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Lighting System Diagnostic System Check performed? | -- | Go to Step 2 | Go to the Lighting System Diagnostic System Check

2

1. Remove the fog lamp switch.
2. With the fog lamps on, test for positive battery voltage at terminal C of the fog lamp connector.

Is positive battery voltage present?

--

Go to Step 3

Go to Step 4

3 | Test for poor connections at the fog lamp switch. Refer to Testing for Intermittent Conditions and Poor Connections in wiring systems. Are poor connections present? | -- | Go to Connector Repairs | Go to Step 5
4 | Repair open in CKT 34. Refer to Wiring Repairs in Wiring Systems. Is repair complete? | -- | System OK | --
5 | Replace the fog lamp switch. Is the repair complete? | -- | System OK | --