Door Lock Switch Replacement. Chevrolet PJJ 2001

For 1990-2009 cars

### Removal Procedure

1. Use a flat-bladed screwdriver in order to pry the power door lock switch (1).
2. Disconnect the wire harness (2) from the power door lock switch (1).
3. Remove the power door lock switch (1).

### Installation Procedure

1. Connect the wire harness (2) to the power door lock switch (1).
2. Install the power door lock switch (1).

Ensure the unit is retained.