Power Steering Pump Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the upper air cleaner and duct. Refer to Air Cleaner Assembly Replacement in Engine Controls - 2.4L.
2. Remove the power steering hoses from the pump. Refer to Power Steering Pressure Hose Replacement (2.4L) and Power Steering Return Hose Replacement (2.4L).
3. Remove the power steering pump mounting bolts (2).
4. Remove the power steering pump (1) from the vehicle.

### Installation Procedure

1. Install the power steering pump (1) to the engine.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the power steering pump mounting bolts (2).

Tighten
Tighten the power steering pump bolts (2) to 26 N·m (19 lb ft).

3. Install the power steering hoses to the pump (1). Refer to Power Steering Pressure Hose Replacement (2.4L) and Power Steering Return Hose Replacement (2.4L).
4. Install the upper air cleaner and duct. Refer to Air Cleaner Assembly Replacement in Engine Controls - 2.4L.
5. Bleed the air from the power steering system. Refer to Bleeding Power Steering System.