Disabling the SIR System. Chevrolet PJJ 2000

For 1990-2009 cars

1. Turn the steering wheel so that the vehicle's wheels are pointing straight ahead.
2. Turn OFF the ignition.
3. Remove the key from the ignition switch.

Important: With the SIR Fuse removed and the ignition ON, the AIR BAG warning lamp illuminates. This is normal operation, and does not indicate an SIR system malfunction.

4. Remove the SIR Fuse from the fuse block.
5. Remove the IP insulator panel. Refer to Instrument Panel Insulator Replacement in Instrument Panel, Gauges and Console.
6. Remove the connector position assurance (CPA) from the driver yellow 2-way connector located at the base of the steering column.
7. Disconnect the driver yellow 2-way connector.
8. Remove the connector position assurance (CPA) from the passenger yellow 2-way connector located near the base of the steering column.
9. Disconnect the passenger yellow 2-way connector.