Upper Extension Trim Panel Replacement. Chevrolet PJJ 2001

For 1990-2009 cars

### Removal Procedure

1. Remove the screw (5).
2. Remove the upper front panel (4).
3. Remove the mirror patch filler (3).

### Installation Procedure

1. Install the mirror patch filler (3).
2. Install the upper front trim finish panel (4).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the screw (5) to the front door upper trim finish panel.

Tighten
Tighten the screw to 1 N·m (12 lb in).