Door Outside Handle Replacement. Chevrolet PJJ 2001

For 1990-2009 cars

### Removal Procedure

1. Lift the front door outside handle (1).
2. Remove the rivets (2) from the front door outside handle.
3. Remove the rod from the front door outside handle (1).
4. Remove the front door outside handle (1).

### Installation Procedure

1. Install the rod to the front door outside handle (1).
2. Install the front door outside handle (1).
3. Lift the front door outside handle (1).
4. Install the rivets (2) to the front door outside handle.