Tilt Spring - Assemble - Off Vehicle. Chevrolet PJJ 2001

For 1990-2009 cars

#### Tools Required

J 41352 Modular Column Holding Fixture

1. Lubricate the spring guide (1) with lithium grease.
2. Install the spring guide (1) into the tilt spring (2).
3. Insert the tilt spring into the steering column support assembly.

Important: The tabs on the spring retainer must fit inside of the steering column support assembly.

4. Secure the tilt spring (2) with the spring retainer (3) by applying pressure to the spring retainer and turning counterclockwise.
5. Release the pressure on the spring retainer (3) once the tabs are locked in place.
6. Remove the steering column and J 41352 from the vise.