Door Water Deflector Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Trim Panel Replacement - Door.
2. Remove the door armrest hanger plate. Refer to Armrest Bracket Replacement.
3. Pull the door water deflector from the door inner panel.

### Installation Procedure

Notice: Proper sealing is necessary in order to prevent water entry into the door and possible damage to inner door components.

1. Apply the sealer to the original sealing areas on the water deflector.
2. Install the water deflector.
3. Install the armrest hanger plate. Refer to Armrest Bracket Replacement.
4. Install the door trim panel. Refer to Trim Panel Replacement - Door.