Hood Primary Latch Striker Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

1. Raise and support the hood.
2. Remove the hood latch striker mounting bolts (4) from the hood latch striker (3).
3. Remove the hood latch striker (3) from the vehicle.

### Installation Procedure

1. Install the hood latch striker (3) to the vehicle.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the hood latch striker mounting bolts (4).

Tighten
Tighten the bolts to 20 N·m (15 lb ft).

3. Adjust the hood. Refer to Hood Adjustment.