Wheel Stud Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 6627-A Wheel Stud Remover

1. Raise the vehicle on a hoist. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the Tire and Wheel Assembly. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
3. Remove the hub and bearing assembly. Refer to Wheel Bearing/Hub Replacement - Front.
4. Remove the wheel stud (1) from the hub and bearing assembly (2) using the J 6627-A Wheel Stud Remover.
5. Discard the stud.

### Installation Procedure

1. Install the replacement stud into the hub and bearing assembly (2).
2. Add enough washers in order to draw the stud into the hub (2).
3. Install the wheel nut (1) with the flat side against the washers (3).
4. Tighten the wheel nut (1) until the wheel stud is fully seated against the hub flange.
5. Back off the wheel nut (1) and remove the washers (3).
6. Install the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
7. Lower the vehicle.