Inline Harness Connector End Views. Chevrolet PJJ 2000

For 1990-2009 cars

Table 1: | In-line Connector C100
Table 2: | In-Line Connector C101
Table 3: | In-Line Connector C102
Table 4: | In-Line Connector C200
Table 5: | In-Line Connector C202
Table 6: | In-Line Connector C203
Table 7: | In-Line Connector C204
Table 8: | In-Line Connector C206
Table 9: | In-Line Connector C207
Table 10: | In-Line Connector C220
Table 11: | In-Line Connector C313 (Wheel Speed Sensors)
Table 12: | In-Line Connector C313 (Fuel System)

#### In-line Connector C100

Connector Part Information

• | 12191487

• | 38-Way M Metri-Pack Mixed Series (BLK)

Connector Part Information

• | 12191499

• | 38-Way F Metri-Pack Mixed Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A2 | PNK | 839 | Fuse Output (Ignition 1) | A2 | PNK | 839 | Fuse Output (Ignition 1)
A4 | LT GRN | 24 | Backup Lamp B | A4 | LT GRN | 24 | Backup Lamp B
A6 | PNK | 639 | Fuse Output (Ignition 1) | A6 | PNK | 639 | Fuse Output (Ignition 1)
A8 | YEL | 5 | Starter Solenoid B (Automatic) | A8 | YEL | 5 | Starter Solenoid B (Automatic)
A8 | PPL | 6 | Starter Solenoid Feed B (Manual) | A8 | PPL | 6 | Fuse Output (Ignition 1)
B1 | PNK | 439 | Fuse Output (Ignition 1) | B1 | PNK | 439 | Fuse Output (Ignition 1)
B3 | ORN | 855 | Fuse Output (ABS) | B3 | ORN | 855 | Fuse Output (ABS)
B7 | -- | -- | Not Used | B7 | -- | -- | Not Used
B9 | GRY | 120 | Fuel Pump Motor Feed | B9 | GRY | 120 | Fuel Pump Motor Feed
C2 | BLK | 884 | Wheel Speed Sensor Signal, Left Front | C2 | BLK | 884 | Wheel Speed Sensor Signal, Left Front
C4 | RED | 885 | Wheel Speed Sensor Return, Left Front | C4 | RED | 885 | Wheel Speed Sensor Return, Left Front
C6 | BRN | 882 | Wheel Speed Sensor Return, Right Front | C6 | BRN | 882 | Wheel Speed Sensor Return, Right Front
C8 | WHT | 883 | Wheel Speed Sensor Signal, Right Front | C8 | WHT | 883 | Wheel Speed Sensor Signal, Right Front
D1 | PPL | 65 | Blower Motor Feed | D1 | PPL | 65 | Blower Motor Feed
D3 | PNK | 1020 | Fuse output (OFF/RUN/CRANK) | D3 | PNK | 1020 | Fuse output (OFF/RUN/CRANK)
D5 | WHT | 1310 | Canister Vent Valve Solenoid Output | D5 | WHT | 1310 | Canister Vent Valve Solenoid Output
D7 | WHT/BLK | 1057 | Sensor Return | D7 | WHT/BLK | 1057 | Sensor Return
D9 | DK GRN | 890 | Fuel Tank Pressure Sensor Signal | D9 | DK GRN | 890 | Fuel Tank Pressure Sensor Signal
E1 | RED | 642 | Fuse Output (Battery) | E1 | RED | 642 | Fuse Output (Battery)
E9 | PPL | 1589 | Secondary Oxygen Sensor Signal | E9 | PPL | 1589 | Secondary Oxygen Sensor Signal
F1 | RED | 242 | Fuse Output (Battery) | F1 | RED | 242 | Fuse Output (Battery)
F9 | RED | 442 | Fuse Output (Battery) | F9 | RED | 442 | Fuse Output (Battery)
G1 | YEL/BLK | 68 | Low Coolant Level Indicator Lamp Output | G1 | YEL/BLK | 68 | Low Coolant Level Indicator Lamp Output
G3 | BRN | 241 | Fuse Output (Ignition 3) | G3 | BRN | 241 | Fuse Output (Ignition 3)
G5 | -- | -- | Not Used | G5 | -- | -- | Not Used
G7 | PPL | 1807 | Serial Data Signal (Class B), 10400 Baud Primary | G7 | PPL | 1807 | Serial Data Signal (Class B), 10400 Baud Primary
G9 | PPL | 1807 | Serial Data Signal (UART), 8192 Baud Primary | G9 | PPL | 1807 | Serial Data Signal (UART), 8192 Baud Primary
H2-H4 | -- | -- | Not Used | H2-H4 | -- | -- | Not Used
H6 | GRY | 705 | Reference Voltage Feed (5 Volt Reference) | H6 | GRY | 705 | Reference Voltage Feed (5 Volt Reference)
H8 | BLK/WHT | 451 | Engine Control Module Ground | H8 | BLK/WHT | 451 | Engine Control Module Ground
J1 | DK GRN | 83 | Cruise Control Signal (DISENGAGE) | J1 | DK GRN | 83 | Cruise Control Signal (DISENGAGE)
J3 | LT BLU/BLK | 396 | Cruise Control Signal (ENGAGE) | J3 | LT BLU/BLK | 396 | Cruise Control Signal (ENGAGE)
J7 | DK GRN/WHT | 817 | Vehicle Speed Signal (4000 Pulses/Mile) | J7 | DK GRN/WHT | 817 | Vehicle Speed Signal (4000 Pulses/Mile)
J9 | PPL | 420 | Brake Pedal Switch Output (Torque Converter Clutch) | J9 | PPL | 420 | Brake Pedal Switch Output (Torque Converter Clutch)
K2 | BRN | 64 | High Speed Blower Relay Feed (Coil) | K2 | BRN | 64 | High Speed Blower Relay Feed (Coil)
K4 | -- | -- | Not Used | K4 | -- | -- | Not Used
K6 | BRN/WHT | 419 | CHECK ENGINE Indicator Output | K6 | BRN/WHT | 419 | CHECK ENGINE Indicator Output
K8 | PNK | 539 | Fuse Output (Ignition 1) | K8 | PNK | 539 | Fuse Output (Ignition 1)

#### In-Line Connector C101

Connector Part Information

• | 12177081

• | 10-Way F Global Terminal 150 Series (BLK)

Connector Part Information

• | 12045808

• | 10-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BRN | 9 | Park Lamp Feed | A | BRN | 9 | Park Lamp Feed
B | PNK | 1200 | High Beam Flash To Pass | B | PNK | 1200 | High Beam Flash To Pass
C | DK BLU | 1201 | Low Beam/Low Beam Headlamp Input | C | DK BLU | 1201 | Low Beam/Low Beam Headlamp Input
D | LT BLU | 1414 | Turn Signal Switch Output Left Front | D | LT BLU | 1414 | Turn Signal Switch Output Left Front
E | DK BLU | 1415 | Turn Signal Switch Output Right Front | E | DK BLU | 1415 | Turn Signal Switch Output Right Front
F | DK GRN | 29 | Horn | F | DK GRN | 29 | Horn
G | -- | -- | Not Used | G | -- | -- | Not Used
H | LT BLU | 14 | LH Front Turn Signal | H | LT BLU | 14 | LH Front Turn Signal
J | BLU | 15 | RH Front Turn Signal | J | BLU | 15 | RH Front Turn Signal
K | -- | -- | Not Used | K | -- | -- | Not Used

#### In-Line Connector C102

Connector Part Information

• | 1216143

• | 4-Way F Metri-Pack 150 Series Sealed (BLK)

Connector Part Information

• | 12110762

• | 4-Way M Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | PNK | 439 | Fuse Output Ignition 1 | A | PNK | 439 | Fuse Output Ignition 1
B | WHT | 1310 | Canister Vent Valve Solenoid Output | B | WHT | 1310 | Canister Vent Valve Solenoid Output
C-D | -- | -- | Not Used | C-D | -- | -- | Not Used

#### In-Line Connector C200

Connector Part Information

• | 12092249

• | 23-Way F Metri-Pack 280 Series (BLK)

Connector Part Information

• | 12092248

• | 23-Way M Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 1240 | Fuse Output (Battery) | A | ORN | 1240 | Fuse Output (Battery)
B | ORN | 340 | Fuse Output (Battery) | B | ORN | 340 | Fuse Output (Battery)
C | BRN | 9 | Park Lamp Feed | C | BRN | 9 | Park Lamp Feed
D | LT BLU | 1662 | Door Adjar Switch Signal, Right Front | D | LT BLU | 1662 | Door Adjar Switch Signal, Right Front
E | DK BLU | 15 | Turn Signal Lamp Feed, Right Front | E | DK BLU | 15 | Turn Signal Lamp Feed, Right Front
F | GRY | 8 | IP Lamp Feed | F | GRY | 8 | IP Lamp Feed
G | BRN | 882 | Wheel Speed Sensor Signal, Right Rear | G | BRN | 882 | Wheel Speed Sensor Signal, Right Rear
H | PPL | 1589 | Secondary Oxygen Sensor Signal | H | PPL | 1589 | Secondary Oxygen Sensor Signal
J | LT GRN | 24 | Backup Lamp Feed | J | LT GRN | 24 | Backup Lamp Feed
K | WHT | 17 | Stop Lamp Switch Output | K | WHT | 17 | Stop Lamp Switch Output
L | -- | -- | Not Used | L | -- | -- | Not Used
M | LT BLU | 1134 | Park Brake Switch Signal | M | LT BLU | 1134 | Park Brake Switch Signal
N | LT BLU | 14 | Turn Signal Lamp Feed, Left Front | N | LT BLU | 14 | Turn Signal Lamp Feed, Left Front
P | WHT | 883 | Wheel Speed Sensor Return, Right Rear | P | WHT | 883 | Wheel Speed Sensor Return, Right Rear
R | -- | -- | Not Used | R | -- | -- | Not Used
S | BLK/WHT | 238 | Seat Belt Switch Signal | S | BLK/WHT | 238 | Seat Belt Switch Signal
T | PNK | 439 | Fuse Output Ignition 1 | T | PNK | 439 | Fuse Output Ignition 1
U | -- | -- | Not Used | U | -- | -- | Not Used
V | WHT | 81 | Power Mirror Motor Feed | V | WHT | 81 | Power Mirror Motor Feed
W | GRY | 120 | Fuel Pump Motor Feed | W | GRY | 120 | Fuel Pump Motor Feed
X | ORN | 1732 | Electronic Control Unit Output (12 Volt), Inadvertent Load Control | X | ORN | 1732 | Electronic Control Unit Output (12 Volt), Inadvertent Load Control
Y | BLK | 884 | Wheel Speed Sensor Signal, Left Rear | Y | BLK | 884 | Wheel Speed Sensor Signal, Left Rear
Z | RED | 885 | Wheel Speed Sensor Return, Left Rear | Z | RED | 885 | Wheel Speed Sensor Return, Left Rear

#### In-Line Connector C202

Connector Part Information

• | 12064752

• | 6-Way F Metri-Pack 280 Series (BLK)

Connector Part Information

• | 12124320

• | 6-Way M Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | WHT | 156 | Courtesy Lamp Output | A | WHT | 156 | Courtesy Lamp Output
B | -- | -- | Not Used | B | -- | -- | Not Used
C | BRN | 141 | Fuse Output (Ignition 3) | C | BRN | 141 | Fuse Output (Ignition 3)
D | BLK | 150 | Ground | D | BLK | 150 | Ground
E | -- | -- | Not Used | E | -- | -- | Not Used
F | ORN | 1732 | Electronic Control Unit Output (12 Volt), Inadvertent Load Control | F | ORN | 1732 | Electronic Control Unit Output (12 Volt), Inadvertent Load Control

#### In-Line Connector C203

Connector Part Information

• | 12047781

• | 3-Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12047782

• | 3-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BRN | 9 | Park Lamp Feed | A | WHT | 9 | Park Lamp Feed
B | BLK | 150 | Ground | B | BLK | 150 | Ground
C | BRN | 243 | Fuse Output Accessory | C | BRN | 141 | Fuse Output Accessory

#### In-Line Connector C204

Connector Part Information

• | 12064998

• | 8-Way Metri-Pack 280 Series (BLK)

Connector Part Information

• | 12066195

• | 8-Way M Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | LT GRN | 66 | Air Conditioning Switch Output | A | LT GRN | 66 | Air Conditioning Switch Output
B | BLK | 150 | Ground | B | BLK | 150 | Ground
C | -- | -- | Not Used | C | -- | -- | Not Used
D | BRN | 41 | Fuse Output (Ignition 3) | D | BRN | 41 | Fuse Output (Ignition 3)
E | PPL | 293 | Rear Defogger Element Feed | E | PPL | 293 | Rear Defogger Element Feed
F | BRN | 64 | Blower Relay Feed (Coil) | F | BRN | 64 | Blower Relay Feed (Coil)
G | PPL | 65 | Blower Motor Feed | G | PPL | 65 | Blower Motor Feed
H | LT BLU | 292 | Rear Defogger Switch Signal Primary | H | LT BLU | 292 | Rear Defogger Switch Signal Primary

#### In-Line Connector C206

Connector Part Information

• | 120092865

• | 2-Way F Metri-Pack 280 Series (YEL)

Connector Part Information

• | 12124901

• | 2-Way M Metri-Pack 280 Series (YEL)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | WHT | 347 | SIR Inflator Feed (Driver) | A | WHT | 347 | SIR Inflator Feed (Driver)
B | DK GRN | 348 | SIR Inflator Output (Driver) | B | DK GRN | 348 | SIR Inflator Output (Driver)

#### In-Line Connector C207

Connector Part Information

• | 12124900

• | 2-Way F Metri-Pack 280 Series (YEL)

Connector Part Information

• | 12110288

• | 2-Way M Metri-Pack 280 Series (YEL)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | WHT/BLK | 1403 | SIR Inflator Feed (Passenger) | A | WHT/BLK | 1403 | SIR Inflator Feed (Passenger)
B | DK GRN/WHT | 1404 | SIR Inflator Output (Passenger) | B | GRN/WHT |  | SIR Inflator Output (Passenger)

#### In-Line Connector C220

Connector Part Information

• | 12089527

• | 6-Way F Metri-Pack 280 Series (GRN)

Connector Part Information

• | 12089745

• | 6-Way M Metri-Pack 280 Series (GRN)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | LT BLU/WHT | 1497 | Power Mirror Select Switch Signal Right Motor | A | LT BLU/WHT | 1497 | Power Mirror Select Switch Signal Right Motor
B | BRN/WHT | 1498 | Power Mirror Feed Right Vertical Motor Up | B | BRN/WHT | 1498 | Power Mirror Feed Right Vertical Motor Up
C | RED/WHT | 881 | Power Mirror Feed Right Horizontal Motor Right | C | RED/WHT | 881 | Power Mirror Feed Right Horizontal Motor Right
D | DK GRN | 890 | Fuel Tank Pressure Sensor Signal | D | DK GRN | 890 | Fuel Tank Pressure Sensor Signal
E | YEL | 88 | Power Mirror Feed Left Vertical Motor Up | E | YEL | 88 | Reference Voltage Feed (5 Volt Reference)
F | YEL/BLK | 910 | Power Mirror Feed | F | YEL/BLK | 910 | Power Mirror Feed

#### In-Line Connector C313 (Wheel Speed Sensors)

Connector Part Information

• | 15317612

• | 1-Way F Metri-Pack 150 Series (GRN)

Connector Part Information

• | 12146439

• | 4-Way M Metri-Pack 150 Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | WHT | 883 | Wheel Speed Sensor Return, Right Rear | A | WHT | 883 | Wheel Speed Sensor Return, Right Rear
B1 | BRN | 882 | Wheel Speed Sensor Signal, Right Rear | B | BRN | 882 | Wheel Speed Sensor Signal, Right Rear
C1 | RED | 885 | Wheel Speed Sensor Return, Left Rear | C | PNK | 885 | Wheel Speed Sensor Return, Left Rear
D1 | BLK | 884 | Wheel Speed Sensor Signal, Left Rear | D | BLK | 884 | Wheel Speed Sensor Signal, Left Rear

#### In-Line Connector C313 (Fuel System)

Connector Part Information

• | 15317612

• | 12-Way F Metri-Pack 150 Series (GRN)

Connector Part Information

• | 15317611

• | 8-Way M Metri-Pack 150 Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A3 | BLK | 150 | Ground | A | BLK | 150 | Ground
B3 | -- | -- | Not Used | B | -- | -- | Not Used
C3 | GRY | 120 | Fuel Pump Motor Feed | C | GRY | 120 | Fuel Pump Motor Feed
D3 | PPL | 1589 | Secondary Oxygen Sensor Signal | D | PPL | 30 | Secondary Oxygen Sensor Signal
E3 | -- | -- | Not Used | E | -- | -- | Not Used
F3 | GRY | 705 | Reference Voltage (5 Volt Reference) | F | GRY/BLK | 416 | Reference Voltage Feed (5 Volt Reference)
G3 | DK GRN | 890 | Fuel Tank Pressure Sensor Signal | G | DK GRN | 890 | Fuel Tank Pressure Sensor Signal
H3 | -- | -- | Not Used | H | -- | -- | Not Used