Front Fog Lamp Replacement. Chevrolet PJJ 2001

For 1990-2009 cars

### Removal Procedure

1. Disconnect the connector from the fog lamp assembly (2).
2. Remove the fog lamp bulb from the fog lamp assembly (2).

Twist and pull outward on the unit.

3. Remove the fog lamp assembly bolts (3).
4. Remove the fog lamp assembly (2) from the fog lamp impact bar (1).

### Installation Procedure

1. Install the fog lamp assembly (2) to the fog lamp impact bar (1).
2. Install the fog lamp assembly bolts (3) in order to secure the fog lamp bracket to the fog lamp impact bar (1).

Tighten
Tighten the fog lamp assembly bolts to 6 N·m (53 lb in).

3. Install the fog lamp bulb to the fog lamp assembly (2).

Ensure the unit is retained.

4. Connect the fog lamp connector to the fog lamp assembly (2).