Electrical Center Identification Views. Chevrolet PJJ 2000

For 1990-2009 cars

### Fuse Block

Fuse/Circuit Breaker | Rating | Description
--- | --- | ---
AIR BG | 15 A | Air Bag
ABS | 10 A | Antilock Brake Solenoids
BCM | 10 A | Body Control Module
BCM/CLU | 10 A | Body Control Module/Cluster
CIG | 15 A | Interior Lamps, Exterior Lamps
CLU BATT | 10 A | Instrument Panel Cluster, Electronic Brake Control Module
CRUISE | 10 A | Cruise Control
ERLS | 10 A | Brake Transaxle Shift Interlock (BTSI), Cruise Control, HVAC: Compressor Control, Multiport Injection
EXT LP | 20 A | Exterior Lamps, Interior Lamps Dimming
FOG LP | 10 A | Daytime Running Lamps: Fog Lamps
F/P-INJ | 15 A | Fuel Pump and Fuel Injectors
FLS-PASS | 20 A | Flash to Pass
HORN | 15 A | Horn
HVAC | 10 A | Antilock Brake, Coolant Fan, HVAC: Compressor Control
IGN MDL | 20 A | Multiport Fuel Injection
MIRRORS | 10 A | Mirrors
O2 HTR | 10 A | Multiport Fuel Injection
PCM | 10 A | Multiport Fuel Injection
PWR ACC | 15 A | Power Door Locks
RDO/INTLP | 25 A* | Radio and Interior Lamp
RFA BATT | 10 A | Keyless Entry
RR DFOG | 30 A | Rear Defogger
STOP/HZD | 20 A | Antilock Brakes, Cruise Control, Exterior Lamps
TURN-BU | 10 A | Back Up Lamps, Exterior Lamps
WIPER | 25 A | Wiper/Washer
PWR WDO (Circuit Breaker) | 25 A | Power Windows
HDLP (Circuit Breaker) | 20 A | Headlamps
REAR DEFOG (Relay) | -- | Rear Defogger Relay

### Underhood Fuse Block

Fuse | Rating | Description
--- | --- | ---
MiniFuse
A/C | 10 A | HVAC: Compressor Control
BLO | 30 A | HVAC: Blower Control and HVAC: Compressor Control
PCM | 10 A | Multiport Fuel Injection
MaxiFuse
ABS | 40 A | Antilock Brakes and Power Distribution
BATT 1 | 40 A | Power Distribution
BATT 2 | 40 A | Power Distribution
COOLING FAN | 30 A | Cooling Fan
IGN | 50 A | Power Distribution, Starter and Charging System