Energy Absorber Pad Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Trim Panel Replacement - Door.
2. Remove the bolts (2).
3. Remove the rear door energy absorber (1).

### Installation Procedure

1. Install the rear door energy absorber (1).
2. Install the bolts (2).

Tighten
Tighten the bolts to 2 N·m (18 lb in).

3. Install the door trim panel. Refer to Trim Panel Replacement - Door.