Diagnostic Trouble Code (DTC) List/Type. Chevrolet PJJ 2000

For 1990-2009 cars

Description | Module
--- | ---
DTC B0016 RF/Passenger Frontal Deployment Loop (Single Stage or Stage 1) Resistance Low | SDM
DTC B0017 RF/Passenger Frontal Deployment Loop (Single Stage or Stage 1) Open | SDM
DTC B0018 RF/Passenger Frontal Deployment Loop (Single Stage or Stage 1) Short to Ground/Voltage Out of Range | SDM
DTC B0022 LF/Driver Frontal Deployment Loop (Single Stage or Stage 1) Resistance Low | SDM
DTC B0024 LF/Driver Frontal Deployment Loop (Single Stage or Stage 1) Short to Ground/Voltage Out of Range | SDM
DTC B0026 LF/Driver Frontal Deployment Loop (Single Stage or Stage 1) Open | SDM
DTC B0035 ADS Closed/Shorted to Ground | SDM
DTC B0036 ADS Open/Missing/Shorted to Battery | SDM
DTC B0051 Deployment Commanded | SDM
DTC B0053 Deployment Commanded with Loop Malfunctions Present | SDM
DTC B1000 ECU Malfunction | SDM
DTC B1001 Option Configuration Error | SDM
DTC U1001-U1254 Loss of XXX Communications | SDM
DTC U1300 Class 2 Data Link Low | SDM
DTC U1301 Class 2 Data Link High | SDM