Body Control Module Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable.
2. Release the BCM Wire Harness Retainer (3) from the BCM Bracket (4).
3. Remove the BCM Bracket Nuts (2).
4. Romove the BCM (1) and BCM Bracket (4) as an assmebly.
5. Remove the BCM (1) from the BCM Braket (4).

### Installation Procedure

1. Install the BCM (1) to the BCM Bracket (4).
2. Install the BCM (1) and BCM Bracket (4) as an assembly.
3. Install the BCM Bracket Nuts (2).

Tighten
Tighten the nuts to 2 N·m (18 in lb).

4. Install the BCM Wire Harness Retainer (3) to the BCM Bracket (4).
5. Connect the negative battery cable.