Air Conditioning (A/C) Compressor and Cooling Fan Relays Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

• | The A/C relay (1)

• | The fuel pump relay (2)

• | The cooling fan relay (3)

1. Remove the underhood fuse block cover (1).
2. Remove the appropriate relay.

• | The A/C relay (1)

• | The fuel pump relay (2)

• | The cooling fan relay (3)

### Installation Procedure

1. Install the following relays.

• | The A/C relay (1)

• | The fuel pump relay (2)

• | The cooling fan relay (3)

2. Install the underhood fuse block cover (1).