Ashtray Lamp Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the console trim plate. Refer to Trim Plate Replacement - Console.
2. Disconnect the electrical connectors.
3. Remove the gear shift handle.
4. Remove the power window switch plate (2).
5. Remove the console. Refer to Console Replacement.
6. Rotate the ashtray lamp socket counter clockwise to remove.
7. Pull the bulb from the socket to remove.

### Installation Procedure

1. Install the bulbs into the sockets.
2. Install the sockets.
3. Connect the electrical connectors.
4. Install the console trim plate. Refer to Trim Plate Replacement - Console.
5. Install the console. Refer to Console Replacement.
6. Install the gear shift handle.
7. Install the power window switch plate (2).