Wheel Stud Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 6627-A Wheel Stud Remover

1. Raise the vehicle on a hoist. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the tire and the wheel assembly. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
3. Remove the brake drum. Refer to Brake Drum Replacement in Drum Brakes.

Notice: Do not hammer on brake drum as damage to the bearing could result.

4. Remove the wheel stud (2) using the J 6627-A Wheel Stud Remover.
5. Discard the wheel stud (2).

### Installation Procedure

1. Install the new stud from the back side of the hub.
2. Install the four flat washers (1) on the hub.
3. Install the wheel nut (2) with the flat side toward the washers (1).
4. Tighten the nut (2) until the stud is properly seated in the hub flange.
5. Remove the nut (2) and the washers (1).
6. Install the brake drum. Refer to Brake Drum Replacement in Drum Brakes.
7. Install the tire and the wheel assembly. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
8. Lower the vehicle.