Sunroof Seal/Molding Replacement. Chevrolet PJJ 2001

For 1990-2009 cars

### Removal Procedure

1. Remove the sunroof window. Refer to Sunroof Glass Panel Replacement
2. Remove the entire weatherstrip by pulling the weatherstrip (1) away from the window (14).

### Installation Procedure

1. Align the butt joint with the center of the sunroof window on the passenger side of the vehicle.
2. Work the weatherstrip into the channel in the window frame.

Continue to work the weatherstrip (1) until the weatherstrip is firmly press fit into the channel.

Install the weatherstrip around the entire sunroof window (14).

3. Install the sunroof window. Refer to Sunroof Glass Panel Replacement