Headlamps Flash to Pass Inoperative. Chevrolet PJJ 2001

For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you perform the Diagnostic System Check - Lighting Systems? | Go to Step 2 | Go to Diagnostic System Check - Lighting Systems
2 | Test for an open in the flash to pass ground circuit. Refer to Circuit Testing and Wiring Repairs in Wiring Systems. Was an open found and corrected? | System OK | Go to Step 3
3 | Inspect for poor connections at the turn/headlamp switch assembly. Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairs in Wiring Systems. Did you find and correct the condition? | System OK | Go to Step 4
4 | Replace the turn/headlamp switch assembly. Refer to Multifunction, Turn Signal, and Hazard Switch Replacement - On Vehicle in Steering Wheel and Column. Is the repair complete? | System OK | --