Rear Compartment Lid Latch Striker Replacement. Chevrolet PJJ 2001

For 1990-2009 cars

### Removal Procedure

1. Remove the lock striker nuts (3).
2. Remove the lock striker reinforcement plate (2).
3. Remove the lock striker (1).

### Installation Procedure

1. Install the lock striker (1).
2. Install the lock striker reinforcement plate (2).
3. Close the compartment lid.
4. Align the compartment lid.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

5. Install the lock striker nuts (3).

Tighten
Tighten the nut to 10 N·m (89 lb in).