Fastener Tightening Specifications. Chevrolet PJJ 2000

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Ball Joint to Steering Knuckle Nut to Install Cotter Pin (Maximum) | 65 N·m plus 180° rotation | 50 lb ft
Ball Joint to Steering Knuckle Nut to Install Cotter Pin (Minimum) | 55 N·m plus 180° rotation | 41 lb ft
Control Arm to Crossmember Bolts (Front Bushing) | 107 N·m | 79 lb ft
Control Arm to Crossmember Bolts (Rear Vertical Bushing) | 170 N·m | 125 lb ft
Front Suspension Crossmember Mounting Bolts | 110 N·m | 71 lb ft
Front Suspension Support Brace Bolts | 17 N·m | 53 lb ft
Hub and Bearing Assembly to Steering Knuckle Bolts | 95 N·m | 70 lb ft
Strut Assembly to Body Bolt | 25 N·m | 18 lb ft
Strut Assembly to Body Nuts | 25 N·m | 18 lb ft
Strut Assembly to Steering Knuckle Nuts | 180 N·m | 133 lb ft
Strut Nut to Strut Rod | 70 N·m | 52 lb ft
Stabilizer Shaft Clamp | 66 N·m | 49 lb ft
Stabilizer Shaft Link to Control Arm Nuts | 17 N·m | 13 lb ft
Tie Rod End to Strut Nut | 20 N·m plus 180° rotation | 15 lb ft plus 180° rotation