Hood Primary and Secondary Latch Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

1. Raise and support the hood.
2. Remove the hood latch cover. Refer to Hood Latch Cover Replacement.
3. Remove the hood latch release cable from the hood latch. Refer to Hood Latch Release Cable Replacement.
4. Remove the hood latch bolts (3) from the hood latch (2).
5. Remove the hood latch (2) from the vehicle.

### Installation Procedure

1. Install the hood latch (2) to the vehicle.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the hood latch bolts (3) to the hood latch (2).

Tighten
Tighten the hood latch bolts to 10 N·m (89 lb in.

3. Install the hood latch release cable to the hood latch. Refer to Hood Latch Release Cable Replacement.
4. Adjust the hood. Refer to Hood Adjustment.