For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Battery

- Battery Cable-to-Battery Terminal Retainer

15 N·m

11 lb ft

- Battery Cable-to-Generator Retaining Nut

8 N·m

71 lb in

- Battery Hold Down Bracket Nuts

8 N·m

71 lb in

- Body Ground Bolt

14 N·m

10 lb ft

- Fuse and Relay Block-to-Inner Fender Bolts

15 N·m

11 lb ft

- Ground Bolt

23 N·m

17 lb ft

- Positive (+) Battery Cable-to-Starter Solenoid Retaining Nut

9 N·m

78 lb in

Charging System

- Brush Holder Screws

2 N·m

18 lb in

- Drive Pulley Retaining Nut

111 N·m

81 lb ft

- End Cover Bolt

4 N·m

35 lb in

- End Cover Nuts

4.5 N·m

39 lb in

- Generator B+ Terminal Retaining Nut

4 N·m

36 lb in

- Generator End Frame Bolts

4.5 N·m

39 lb in

- Generator Front Bearing Retainer Screws

3 N·m

27 lb in

- Generator Lower Mounting Bolt

54 N·m

40 lb ft

- Generator Upper Mounting Bolt

25 N·m

18 lb ft

- Generator Rectifier Screws

3 N·m

26 lb in

- Voltage Regulator Screws

2 N·m

18 lb in

Cranking System

- Field Frame End Cover Bolts

1.5 N·m

13 lb in

- Positive (+) Battery Cable-to-Starter Solenoid Retaining Nut

9 N·m

78 lb in

- Solenoid End Cover Bolts

6 N·m

53 lb in

- Solenoid Lead Wire Nut

6 N·m

53 lb in

- Solenoid Terminal Nuts

17 N·m

12 lb ft

- Starter Drive Housing Bolts

6 N·m

52 lb in

- Starter Motor Mounting Bolts

37 N·m

27 lb ft

- Starter Through Bolts

6 N·m

52 lb in

Ignition System

- Ignition Coil Bolts

9 N·m

78 lb in

- Spark Plugs

18 N·m

13 lb ft