For 1990-2009 cars

#### Tools Required

• | J 26941 Countershaft Bearing and Drive Axle Seal Remover

• | J 2619-01 Slide Hammer

1. Remove the 3 bolts and the 3 fluid pipe clamps (1) from the torque converter housing (3).
2. Remove the 2 fluid pipes (2) from the torque converter housing (1).
3. Remove the bolt and the countershaft front roller bearing retainer (3) from the torque converter housing (1).
4. Use the J 26941 with a J 2619-01 in order to remove the countershaft front roller bearing (1) from the torque converter housing (2).
5. Remove the countershaft lubrication seal (2) from the countershaft front roller bearing bore (1).
6. Use the J 26941 with a J 2619-01 in order to remove the right drive axle shaft fluid seal from the torque converter housing.
7. Use the J 26941 with a J 2619-01 in order to remove the following components from the torque converter housing (1):

• | The right differential side bearing race (2)

• | The right differential selective shim (3)

8. Clean the sealant from the torque converter housing-to-transaxle case mating surfaces.